(footprint "Mini-Circuits_BK377_LandPatternPL-005"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case BK377 (https://ww2.minicircuits.com/case_style/BK276.pdf) according to land-pattern PL-005, including GND vias (https://ww2.minicircuits.com/pcb/98-pl005.pdf)")
	(tags "Mini-circuits VCXO JTOS PL-005")
	(property "Reference" "REF**"
		(at 0 -11.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_BK377_LandPatternPL-005"
		(at 0 11.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -7.4803 -7.62)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -7.4803 -2.54)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -7.4803 0)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -7.4803 5.08)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -7.4803 7.62)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -7.4041 -7.62)
		(size 1.4732 1.651)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -7.4041 -1.27)
		(size 1.4732 4.191)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -7.4041 6.35)
		(size 1.4732 4.191)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -6.6675 -7.62)
		(size 2.54 1.651)
		(drill
			(offset 1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -4.953 -7.62)
		(size 3.429 1.651)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -4.953 -1.27)
		(size 3.429 4.191)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -4.953 6.35)
		(size 3.429 4.191)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.6543 -7.62)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.6543 -5.08)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.6543 -2.54)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.6543 0)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.6543 2.54)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.6543 5.08)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.6543 7.62)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 0 0)
		(size 6.477 16.891)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.6543 -7.62)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.6543 -5.08)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.6543 -2.54)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.6543 0)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.6543 2.54)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.6543 5.08)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.6543 7.62)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 4.953 -7.62)
		(size 3.429 1.651)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 4.953 2.54)
		(size 3.429 11.811)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 7.4041 -7.62)
		(size 1.4732 1.651)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 7.4041 2.54)
		(size 1.4732 11.811)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 7.4803 -7.62)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 7.4803 -2.54)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 7.4803 0)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 7.4803 2.54)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 7.4803 5.08)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 7.4803 7.62)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at -5.3975 -5.08)
		(size 2.54 1.651)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.889)
		(zone_connect 2)
	)
	(pad "3" smd rect
		(at -6.6675 -2.54)
		(size 2.54 1.651)
		(drill
			(offset 1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at -6.6675 0)
		(size 2.54 1.651)
		(drill
			(offset 1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "5" smd rect
		(at -5.3975 2.54)
		(size 2.54 1.651)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.889)
		(zone_connect 2)
	)
	(pad "6" smd rect
		(at -6.6675 5.08)
		(size 2.54 1.651)
		(drill
			(offset 1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "7" smd rect
		(at -6.6675 7.62)
		(size 2.54 1.651)
		(drill
			(offset 1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "8" smd rect
		(at 6.6675 7.62)
		(size 2.54 1.651)
		(drill
			(offset -1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "9" smd rect
		(at 6.6675 5.08)
		(size 2.54 1.651)
		(drill
			(offset -1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "10" smd rect
		(at 6.6675 2.54)
		(size 2.54 1.651)
		(drill
			(offset -1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "11" smd rect
		(at 6.6675 0)
		(size 2.54 1.651)
		(drill
			(offset -1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "12" smd rect
		(at 6.6675 -2.54)
		(size 2.54 1.651)
		(drill
			(offset -1.27 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "13" smd rect
		(at 5.3975 -5.08)
		(size 2.54 1.651)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.889)
		(zone_connect 2)
	)
	(pad "14" smd rect
		(at 5.3975 -7.62)
		(size 2.54 1.651)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_BK377.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
