(footprint "Mini-Circuits_CD542_LandPatternPL-094"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for mini circuit case CD542, Land pattern PL-094, pads 5 and 2 connected via insulated copper area below body, vias included (case drawing: https://ww2.minicircuits.com/case_style/CD542.pdf, land pattern drawing: https://ww2.minicircuits.com/pcb/98-pl094.pdf)")
	(tags "mini-circuits CD542 pl-094")
	(property "Reference" "REF**"
		(at 0.004446 -4.953 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_CD542_LandPatternPL-094"
		(at 0 5.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.54 -2.54 270)
		(size 1.651 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(pad "2" thru_hole circle
		(at -4.4958 0 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at -4.3815 0 270)
		(size 1.651 1.143)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at -2.54 0 270)
		(size 1.651 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at -0.9525 0 270)
		(size 1.651 0.635)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 -2.54 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 -1.27 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 0 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at 0 0 270)
		(size 6.731 1.27)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 1.27 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 2.54 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" smd rect
		(at -2.54 2.54 270)
		(size 1.651 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(pad "4" smd rect
		(at 2.54 2.54 270)
		(size 1.651 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(pad "5" smd rect
		(at 0.9525 0 270)
		(size 1.651 0.635)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "5" smd rect
		(at 2.54 0 270)
		(size 1.651 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "5" smd rect
		(at 4.3815 0 270)
		(size 1.651 1.143)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "5" thru_hole circle
		(at 4.4958 0 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "6" smd rect
		(at 2.54 -2.54 270)
		(size 1.651 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_CD542.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
