(footprint "Mini-Circuits_CK605"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case CK605 (https://ww2.minicircuits.com/case_style/CK605.pdf)")
	(tags "Mini-Circuits CK605")
	(property "Reference" "REF**"
		(at -5.08 -8.128 180)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_CK605"
		(at 0 8.0772 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.096 -3.429 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.096 -0.889 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.096 1.651 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -6.096 4.191 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.429 6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.889 6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.651 6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.191 6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 6.096 3.302 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 6.096 0.762 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.096 -1.778 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 6.096 -4.318 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 4.191 -6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.651 -6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.889 -6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3.429 -6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_CK605.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
