(footprint "Mini-Circuits_CK605_LandPatternPL-012"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case CK605 (https://ww2.minicircuits.com/case_style/CK605.pdf) following land pattern PL-012, including GND vias (https://ww2.minicircuits.com/pcb/98-pl012.pdf)")
	(tags "Mini-Circuits PL-012")
	(property "Reference" "REF**"
		(at -5.08 -8.128 180)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_CK605_LandPatternPL-012"
		(at 0 8.0772 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -6.096 -4.699)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -6.096 -3.429 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -6.096 2.921)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -4.699 -6.096)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -4.699 -3.429)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -4.699 1.651)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -4.699 4.191)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -4.699 6.096)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -3.556 -2.159)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -3.556 0.381)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -3.4925 -4.7625)
		(size 6.731 4.191)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -3.429 -4.699)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -3.429 4.699)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.159 -6.096)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.159 6.096)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -1.27 3.8735)
		(size 11.176 5.969)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -0.889 -4.699)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -0.889 4.699)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 0 -0.889)
		(size 8.636 3.556)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 0.381 -3.556)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 0.381 6.096)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 1.651 -3.4925)
		(size 3.556 1.651)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 1.651 4.699)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.921 -3.556)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.921 6.096)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 3.556 -0.508)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 3.556 2.032)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 4.191 4.699)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 4.699 -4.699)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 4.699 -1.778)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 4.699 3.302)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 5.1435 -3.937)
		(size 3.429 5.842)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 5.461 -6.096)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 5.461 6.096)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 5.588 4.699)
		(size 2.54 4.318)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 6.096 -3.048)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 6.096 4.572)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at -6.096 -0.889 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 1.016)
	)
	(pad "3" smd rect
		(at -6.096 1.651 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at -6.096 4.191 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "5" smd rect
		(at -3.429 6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "6" smd rect
		(at -0.889 6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "7" smd rect
		(at 1.651 6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "8" smd rect
		(at 4.191 6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "9" smd rect
		(at 6.096 3.302 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "10" smd rect
		(at 6.096 0.762 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 1.016)
	)
	(pad "11" smd rect
		(at 6.096 -1.778 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "12" smd rect
		(at 6.096 -4.318 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "13" smd rect
		(at 4.191 -6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "14" smd rect
		(at 1.651 -6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 1.016)
	)
	(pad "15" smd rect
		(at -0.889 -6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "16" smd rect
		(at -3.429 -6.096 270)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_CK605.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
