(footprint "Mini-Circuits_GP1212_LandPatternPL-176"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case GP1212 (https://ww2.minicircuits.com/case_style/GP731.pdf) following land pattern PL-176, including GND vias (https://www.minicircuits.com/pcb/98-pl176.pdf)")
	(tags "mini-circuits PL-176")
	(property "Reference" "REF**"
		(at 0 -5.969 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_GP1212_LandPatternPL-176"
		(at 0 6.096 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -4.445 -4.445)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -4.445 4.445)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -4.064 -1.905 180)
		(size 1.778 1.016)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -3.683 -3.175)
		(size 2.54 3.556)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -3.683 3.175)
		(size 2.54 3.556)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -1.27 -1.27)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -1.27 1.27)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 0 0)
		(size 4.826 9.906)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 1.27 -1.27)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 1.27 1.27)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 3.683 -3.175)
		(size 2.54 3.556)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 3.683 3.175)
		(size 2.54 3.556)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 4.445 -4.445)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 4.445 4.445)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at -4.064 0 180)
		(size 1.778 1.016)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.762)
	)
	(pad "3" smd rect
		(at -4.064 1.905 180)
		(size 1.778 1.016)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 0 4.064 270)
		(size 1.778 1.016)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "5" smd rect
		(at 4.064 1.905)
		(size 1.778 1.016)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "6" smd rect
		(at 4.064 0)
		(size 1.778 1.016)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.762)
	)
	(pad "7" smd rect
		(at 4.064 -1.905)
		(size 1.778 1.016)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "8" smd rect
		(at 0 -4.064 270)
		(size 1.778 1.016)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_GP1212.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
