(footprint "Mini-Circuits_HF1139_LandPatternPL-230"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case HF1139 (https://ww2.minicircuits.com/case_style/HF1139.pdf) following land pattern PL-230, including GND vias (https://ww2.minicircuits.com/pcb/98-pl230.pdf)")
	(tags "Mini-Circuits PL-230")
	(property "Reference" "REF**"
		(at 0 -10.922 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_HF1139_LandPatternPL-230"
		(at 0 10.922 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.1905 0 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.2705 -7.62 270)
		(size 1.524 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 3.3782)
	)
	(pad "2" smd rect
		(at 5.2705 -7.62 270)
		(size 1.524 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 6.35 -8.382 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 6.35 -6.858 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -6.35 -3.302 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -6.35 -1.778 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" smd rect
		(at -5.2705 -2.54 270)
		(size 1.524 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 5.2705 -2.54 270)
		(size 1.524 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 6.35 -3.302 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 6.35 -1.778 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "5" thru_hole circle
		(at -6.35 1.778 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "5" thru_hole circle
		(at -6.35 3.302 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "5" smd rect
		(at -5.2705 2.54 270)
		(size 1.524 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "6" smd rect
		(at 5.2705 2.54 270)
		(size 1.524 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "6" thru_hole circle
		(at 6.35 1.778 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "6" thru_hole circle
		(at 6.35 3.302 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -6.35 6.858 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -6.35 8.382 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" smd rect
		(at -5.2705 7.62 270)
		(size 1.524 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "7" smd rect
		(at -4.0259 2.794 270)
		(size 13.208 5.6642)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -0.635 -7.62 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -0.635 -5.08 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -0.635 -2.54 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -0.635 0 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -0.635 2.54 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -0.635 5.08 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at -0.635 7.62 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" smd rect
		(at 0 0 270)
		(size 18.796 2.3876)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at 0.635 -7.62 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at 0.635 -5.08 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at 0.635 -2.54 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at 0.635 0 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at 0.635 2.54 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at 0.635 5.08 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" thru_hole circle
		(at 0.635 7.62 270)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "7" smd rect
		(at 4.0259 -2.794 270)
		(size 13.208 5.6642)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "8" smd rect
		(at 5.2705 7.62 270)
		(size 1.524 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 3.3782)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_HF1139.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
