(footprint "Mini-Circuits_HZ1198"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case HZ1198 (https://ww2.minicircuits.com/case_style/HZ1198.pdf)")
	(tags "Mini-Circuits HZ1198")
	(property "Reference" "REF**"
		(at 0 -8.128 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_HZ1198"
		(at -0.1 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.2 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.9977 -5.6515)
		(size 2.9972 1.7018)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 6.9977 -5.6515)
		(size 2.9972 1.7018)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 9.779 0)
		(size 2.4384 1.9812)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 6.8961 5.2578)
		(size 1.9812 2.4892)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -6.8961 5.2578)
		(size 1.9812 2.4892)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -9.779 0)
		(size 2.4384 1.9812)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_HZ1198.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
