(footprint "Mini-Circuits_HZ1198_LandPatternPL-247"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits cas HZ1198 (https://ww2.minicircuits.com/case_style/HZ1198.pdf) following land pattern PL-247, including GND-vias (https://www.minicircuits.com/pcb/98-pl247.pdf)")
	(tags "Mini-Circuits PL-247 HZ1198")
	(property "Reference" "REF**"
		(at -0.254 -8.3032 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_HZ1198_LandPatternPL-247"
		(at -0.1 7.7968 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -0.0032 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.9977 -5.8547)
		(size 2.9972 1.7018)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.8128)
	)
	(pad "2" smd rect
		(at 6.9977 -5.8547)
		(size 2.9972 1.7018)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.8128)
	)
	(pad "3" thru_hole circle
		(at -8.89 -2.7432)
		(size 0.762 0.762)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -8.89 2.3368)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -8.89 4.8768)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -6.35 -2.7432)
		(size 0.762 0.762)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -6.35 -0.2032)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -6.35 2.3368)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -3.81 -5.2832)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -3.81 -2.7432)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -3.81 -0.2032)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -3.81 2.3368)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -3.81 4.8768)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -1.27 -5.2832)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -1.27 -2.7432)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -1.27 -0.2032)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -1.27 2.3368)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at -1.27 4.8768)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" smd rect
		(at 0 -5.207)
		(size 9.3726 4.064)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "3" smd rect
		(at 0 1.8034)
		(size 23.0124 10.0076)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 1.27 -5.2832)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 1.27 -2.7432)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 1.27 -0.2032)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 1.27 2.3368)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 1.27 4.8768)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 3.81 -5.2832)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 3.81 -2.7432)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 3.81 -0.2032)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 3.81 2.3368)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 3.81 4.8768)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 6.35 -2.7432)
		(size 0.762 0.762)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 6.35 -0.2032)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 6.35 2.3368)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 8.89 -2.7432)
		(size 0.762 0.762)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 8.89 2.3368)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" thru_hole circle
		(at 8.89 4.8768)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" smd rect
		(at 9.779 -0.2032)
		(size 2.4384 1.9812)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 6.8961 5.0546)
		(size 1.9812 2.4892)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "5" smd rect
		(at -6.8961 5.0546)
		(size 1.9812 2.4892)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "6" smd rect
		(at -9.779 -0.2032)
		(size 2.4384 1.9812)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_HZ1198.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
