(footprint "Mini-Circuits_QQQ130_LandPattern_PL-236_ClockwisePinNumbering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case QQQ130 (https://ww2.minicircuits.com/case_style/QQQ130.pdf) following land pattern PL-236, including GND vias (https://ww2.minicircuits.com/pcb/98-pl236.pdf)")
	(tags "Mini-Circuits PL-236")
	(property "Reference" "REF**"
		(at -5.207 0 90)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_QQQ130_LandPattern_PL-236_ClockwisePinNumbering"
		(at 0 7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.54 -3.81)
		(size 1.524 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at -2.54 -1.9685 90)
		(size 0.635 1.524)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.54 -0.8255)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.54 0.8255)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 0 -0.8255)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" smd rect
		(at 0 0 90)
		(size 3.3274 6.604)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 0 0.8255)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.54 -0.8255)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.54 0.8255)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at 0 -3.81)
		(size 1.524 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(pad "3" smd rect
		(at 2.54 -3.81)
		(size 1.524 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(pad "4" smd rect
		(at 2.54 3.81)
		(size 1.524 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(pad "5" smd rect
		(at 0 3.81)
		(size 1.524 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(pad "6" smd rect
		(at -2.54 3.81)
		(size 1.524 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.635)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_QQQ130.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
