(footprint "Mini-Circuits_TT1224_LandPatternPL-258_ClockwisePinNumbering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case TT1224 (https://ww2.minicircuits.com/case_style/TT1224.pdf) following land-pattern PL-258, including GND-vias (https://www.minicircuits.com/pcb/98-pl258.pdf)")
	(tags "PL-258 Mini-Circuits")
	(property "Reference" "REF**"
		(at 0 -5.207 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_TT1224_LandPatternPL-258_ClockwisePinNumbering"
		(at -0.127 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.54 -2.9845 270)
		(size 1.651 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.9398)
	)
	(pad "2" thru_hole circle
		(at -2.54 0 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at -2.54 1.651 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at -2.54 4.318 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at -1.27 0 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at -1.27 1.651 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at -1.27 2.7305 90)
		(size 4.191 4.064)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at -1.27 4.318 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 -4.318 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at 0 -2.9845 270)
		(size 1.651 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 -1.651 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 0 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at 0 0 90)
		(size 1.27 6.604)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 1.651 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 0 4.318 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 1.27 -4.318 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" smd rect
		(at 1.27 -2.7305 90)
		(size 4.191 4.064)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 1.27 -1.651 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 1.27 0 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 2.54 -4.318 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 2.54 -1.651 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "2" thru_hole circle
		(at 2.54 0 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "3" smd rect
		(at 2.54 -2.9845 270)
		(size 1.651 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 2.54 2.9845 90)
		(size 1.651 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.9398)
	)
	(pad "5" smd rect
		(at 0 2.9845 90)
		(size 1.651 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "6" smd rect
		(at -2.54 2.9845 90)
		(size 1.651 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_TT1224.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
