(footprint "Mini-Circuits_TTT167_LandPatternPL-079"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case TTT167 (Mini-Circuits_TTT167_LandPatternPL-079) following land pattern PL-079, including GND vias (https://ww2.minicircuits.com/pcb/98-pl079.pdf)")
	(tags "Mini-Circuits PL-079")
	(property "Reference" "REF**"
		(at 0 -7 180)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_TTT167_LandPatternPL-079"
		(at 0 6.985 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.969 0)
		(size 1.778 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 1.143)
	)
	(pad "2" smd rect
		(at 5.969 0 180)
		(size 1.778 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 1.143)
	)
	(pad "3" smd rect
		(at 0 -4.3815 270)
		(size 1.778 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 1.143)
	)
	(pad "4" thru_hole circle
		(at -6.604 -3.81 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -6.604 -2.54 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -6.604 2.54 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -6.604 3.81 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -5.715 -5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -5.08 5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -3.175 -5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -3.175 -0.635 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -3.175 0.635 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -3.175 5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at -1.905 -5.588 180)
		(size 5.207 3.683)
		(drill
			(offset 2.6035 -1.8415)
		)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -1.27 5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -0.635 -1.27 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at -0.635 2.54 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 0 0 180)
		(size 7.62 4.4704)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 0 4.3815 90)
		(size 1.778 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 0 5.588 180)
		(size 14.224 3.683)
		(drill
			(offset 0 1.8415)
		)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 0.635 -1.27 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 0.635 2.54 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 1.27 5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3.175 -5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3.175 -0.635 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3.175 0.635 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 3.175 5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 5.08 5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 5.715 -5.08 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 6.604 -3.81 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 6.604 -2.54 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 6.604 2.54 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" thru_hole circle
		(at 6.604 3.81 90)
		(size 1.016 1.016)
		(drill 0.508)
		(layers "*.Cu")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 7.112 -5.588 180)
		(size 5.207 3.683)
		(drill
			(offset 2.6035 -1.8415)
		)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "5" smd rect
		(at 4.445 -4.3815 270)
		(size 1.778 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "6" smd rect
		(at -4.445 -4.3815 270)
		(size 1.778 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_TTT167.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
