(footprint "Astrocast_AST50147-00"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "L-band satellite communication module, https://docs.astrocast.com/dl/0532-DOC-M2M-ASTRO-Astronode_S-Datasheet.pdf")
	(tags "RF module Astrocast radio Astronode")
	(property "Reference" "REF**"
		(at -10.16 -19.05 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Astrocast_AST50147-00"
		(at 0 -15.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -15.25 -15.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "2" smd roundrect
		(at -15.25 -14.23)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "3" smd roundrect
		(at -15.25 -12.96)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "4" smd roundrect
		(at -15.25 -11.69)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "5" smd roundrect
		(at -15.25 -10.42)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "6" smd roundrect
		(at -15.25 -9.15)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "7" smd roundrect
		(at -15.25 -7.88)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "8" smd roundrect
		(at -15.25 -6.61)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "9" smd roundrect
		(at -15.25 -5.34)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "10" smd roundrect
		(at -15.25 -4.07)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "11" smd roundrect
		(at -15.25 -2.8)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "12" smd roundrect
		(at -15.25 -1.53)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "13" smd roundrect
		(at -15.25 -0.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "14" smd roundrect
		(at -15.25 1.01)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "15" smd roundrect
		(at -15.25 2.28)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "16" smd roundrect
		(at -15.25 3.55)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "17" smd roundrect
		(at -15.25 4.82)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "18" smd roundrect
		(at -15.25 6.09)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "19" smd roundrect
		(at -15.25 7.36)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "20" smd roundrect
		(at 15.25 7.36)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "21" smd roundrect
		(at 15.25 6.09)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "22" smd roundrect
		(at 15.25 4.82)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "23" smd roundrect
		(at 15.25 3.55)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "24" smd roundrect
		(at 15.25 2.28)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "25" smd roundrect
		(at 15.25 1.01)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "26" smd roundrect
		(at 15.25 -0.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "27" smd roundrect
		(at 15.25 -1.53)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "28" smd roundrect
		(at 15.25 -2.8)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "29" smd roundrect
		(at 15.25 -4.07)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "30" smd roundrect
		(at 15.25 -5.34)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "31" smd roundrect
		(at 15.25 -6.61)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "32" smd roundrect
		(at 15.25 -7.88)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "33" smd roundrect
		(at 15.25 -9.15)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "34" smd roundrect
		(at 15.25 -10.42)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "35" smd roundrect
		(at 15.25 -11.69)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "36" smd roundrect
		(at 15.25 -12.96)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "37" smd roundrect
		(at 15.25 -14.23)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "38" smd roundrect
		(at 15.25 -15.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "Tracks, vias and pads Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -15.55 -16) (xy -14.45 -16) (xy -14.45 7.86) (xy -15.55 7.86) (xy -15.55 17.55) (xy 15.55 17.55)
				(xy 15.55 7.86) (xy 14.45 7.86) (xy 14.45 -16) (xy 15.55 -16) (xy 15.55 -17.55) (xy -15.55 -17.55)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Astrocast_AST50147-00.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
