(footprint "BM78SPPS5xC2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Bluetooth Dual-mode module with integral chip antenna (http://ww1.microchip.com/downloads/en/DeviceDoc/60001380C.pdf)")
	(tags "Bluetooth BR/EDR BLE")
	(property "Reference" "REF**"
		(at -6.12 -12 180)
		(layer "F.SilkS")
	)
	(property "Value" "BM78SPPS5xC2"
		(at -0.1 12.54 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEP OUT ZONE"
		(at 0 -9 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.75 -10.2 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -5.75 -9.1 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -5.75 -2.9 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.75 -1.8 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.75 -0.7 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -5.75 0.4 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -5.75 1.5 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -5.75 2.6 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -5.75 3.7 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -5.75 4.8 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -5.75 5.9 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -5.75 7 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -5.75 8.1 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -5.75 9.2 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -3.3 10.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -2.2 10.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.1 10.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 0 10.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.1 10.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.2 10.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 3.3 10.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 5.75 9.2 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 5.75 8.1 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 5.75 7 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 5.75 5.9 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 5.75 4.8 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 5.75 3.7 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 5.75 2.6 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 5.75 1.5 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 5.75 0.4 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 5.75 -0.7 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 5.75 -9.1 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 5.75 -10.2 270)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 6 -10.55) (xy 5 -10.55) (xy 5 -9.85) (xy 6 -9.85) (xy 6 -9.45) (xy 5 -9.45) (xy 5 -8.75) (xy 6 -8.75)
				(xy 6 -3.8) (xy 2 -3.8) (xy 2 -7) (xy -6 -7) (xy -6 -8.75) (xy -5 -8.75) (xy -5 -9.45) (xy -6 -9.45)
				(xy -6 -9.85) (xy -5 -9.85) (xy -5 -10.55) (xy -6 -10.55) (xy -6 -11) (xy 6 -11)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/BM78SPPS5xC2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
