(footprint "Digi_XBee_SMT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.digi.com/resources/documentation/digidocs/pdfs/90002126.pdf http://ftp1.digi.com/support/documentation/90001020_F.pdf")
	(tags "Digi XBee SMT RF")
	(property "Reference" "REF**"
		(at 0 -18.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "Digi_XBee_SMT"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Below module keepout or"
		(at 0 -4.2 0)
		(layer "Dwgs.User")
	)
	(fp_text user "GND plane recommended!"
		(at 0 -3 0)
		(layer "Dwgs.User")
	)
	(fp_text user "required"
		(at 4.8 -9 0)
		(layer "Cmts.User")
	)
	(fp_text user "Keepout"
		(at 4.8 -10 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.25 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -11 -9.9)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -11 -7.9)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -11 -5.9)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -11 -3.9)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -11 -1.9)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -11 0.1)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -11 2.1)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -11 4.1)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -11 6.1)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -11 8.1)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -11 10.1)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -11 12.1)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -11 14.1)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -7 15.93 90)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -5 15.93 90)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3 15.93 90)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1 15.93 90)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1 15.93 90)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 3 15.93 90)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 5 15.93 90)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 7 15.93 90)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 11 14.08)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 11 12.08)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 11 10.08)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 11 8.08)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 11 6.08)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 11 4.08)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 11 2.08)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 11 0.08)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 11 -1.92)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 11 -3.92)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 11 -5.92)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 11 -7.92)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 11 -9.92)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 11 -11.92)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 11 -13.92)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 11 -15.92)
		(size 2.84 1.52)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 3 -10.6) (xy 9.4 -10.6) (xy 9.4 -8.3) (xy 3 -8.3)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Digi_XBee_SMT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
