(footprint "ESP32-C3-WROOM-02U"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "RF Module, ESP32-C3 WROOM-02 , Wi-Fi and Bluetooth, BLE, external antenna, https://www.espressif.com/sites/default/files/documentation/esp32-c3-wroom-02_datasheet_en.pdf")
	(tags "ESP32-C3 WROOM-02 espressif")
	(property "Reference" "REF**"
		(at 0 -8.3 180)
		(layer "F.SilkS")
	)
	(property "Value" "ESP32-C3-WROOM-02U"
		(at 0 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.14 -0.9)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.14 0.2)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.14 1.3)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.96 -0.9)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.96 0.2)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.96 1.3)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.06 -0.9)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.06 0.2)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.06 1.3)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -8.75 -6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8.75 -4.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -8.75 -3)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -8.75 -1.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -8.75 0)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -8.75 1.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.75 3)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8.75 4.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -8.75 6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 8.75 6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 8.75 4.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 8.75 3)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 8.75 1.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 8.75 0)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 8.75 -1.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 8.75 -3)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 8.75 -4.5)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 8.75 -6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" thru_hole circle
		(at -0.14 -0.35)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at -0.14 0.75)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 0.41 -0.9)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 0.41 0.2)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 0.41 1.3)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 0.96 -0.35)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" smd rect
		(at 0.96 0.2)
		(size 2.9 2.9)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 0.96 0.75)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 1.51 -0.9)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 1.51 0.2)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 1.51 1.3)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 2.06 -0.35)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "19" thru_hole circle
		(at 2.06 0.75)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-C3-WROOM-02U.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
