(footprint "ESP32-S2-MINI-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2.4 GHz Wi-Fi and Bluetooth combo chip, external antenna, https://www.espressif.com/sites/default/files/documentation/esp32-s3-mini-1_mini-1u_datasheet_en.pdf")
	(tags "2.4 GHz Wi-Fi Bluetooth external antenna espressif  20*15.4mm")
	(property "Reference" "REF**"
		(at -5.95 11.85 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "ESP32-S2-MINI-1"
		(at 0 3.55 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Keepout Area"
		(at -0.01 -15.36 0)
		(layer "Cmts.User")
	)
	(fp_text user "Antenna"
		(at 0 -7.675 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 5.05 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7 -3.4)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -7 -2.55)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -7 -1.7)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -7 -0.85)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -7 0)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -7 0.85)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -7 1.7)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -7 2.55)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -7 3.4)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -7 4.25)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -7 5.1)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -7 5.95)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -7 6.8)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -7 7.65)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -7 8.5)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -5.95 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -5.1 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -4.25 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -3.4 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -2.55 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.7 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -0.85 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 0 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0.85 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 1.7 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 2.55 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 3.4 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 4.25 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 5.1 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 5.95 9.55 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 7 8.5)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 7 7.65)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 7 6.8)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 7 5.95)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 7 5.1)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 7 4.25)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 7 3.4)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 7 2.55)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 7 1.7)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 7 0.85)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 7 0)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 7 -0.85)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 7 -1.7)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 7 -2.55)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 7 -3.4)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 5.95 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 5.1 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 4.25 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 3.4 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 2.55 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 1.7 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 0.85 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 0 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at -0.85 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -1.7 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -2.55 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -3.4 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -4.25 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -5.1 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at -5.95 -4.45 90)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd roundrect
		(at -1.65 0.9)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.33)
		(chamfer top_left)
		(zone_connect 2)
	)
	(pad "61" smd rect
		(at -1.65 2.55)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "61" smd rect
		(at -1.65 4.2)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "61" smd rect
		(at 0 0.9)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "61" smd rect
		(at 0 2.55)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "61" smd rect
		(at 0 4.2)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "61" smd rect
		(at 1.65 0.9)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "61" smd rect
		(at 1.65 2.55)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "61" smd rect
		(at 1.65 4.2)
		(size 1.2 1.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "62" smd rect
		(at -7 -4.45)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at -7 9.55)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at 7 9.55)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at 7 -4.45)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "Antenna")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 22.7 -5.25) (xy -22.7 -5.25) (xy -22.7 -24.75) (xy 22.7 -24.75)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-S2-MINI-1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
