(footprint "ESP32-S2-WROVER"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ESP32-S2-WROVER(-I) 2.4 GHz Wi-Fi https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf")
	(tags "ESP32-S2  ESP32  WIFI")
	(property "Reference" "REF**"
		(at -10.41 10.53 90)
		(layer "F.SilkS")
	)
	(property "Value" "ESP32-S2-WROVER"
		(at 0.04 13.145 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEP-OUT ZONE"
		(at 0 -27.09 0)
		(layer "Cmts.User")
	)
	(fp_text user "ANTENNA"
		(at 0 -16.15 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.52 -5.065)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "" smd roundrect
		(at -2.52 -3.735)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "" smd roundrect
		(at -2.52 -2.405)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "" smd roundrect
		(at -1.19 -5.065)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "" smd roundrect
		(at -1.19 -3.735)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "" smd roundrect
		(at -1.19 -2.405)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "" smd roundrect
		(at 0.14 -5.065)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "" smd roundrect
		(at 0.14 -3.735)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "" smd roundrect
		(at 0.14 -2.405)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.233645)
	)
	(pad "1" smd rect
		(at -8.625 -11.775)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8.625 -10.275)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -8.625 -8.775)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -8.625 -7.275)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -8.625 -5.775)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -8.625 -4.275)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.625 -2.775)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8.625 -1.275)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -8.625 0.225)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -8.625 1.725)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -8.625 3.225)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -8.625 4.725)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -8.625 6.225)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -8.625 7.725)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -8.625 9.225 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -8.625 10.725 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -6.75 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -5.25 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -3.75 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -2.25 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -0.75 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 0.75 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 2.25 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 3.75 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 5.25 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 6.75 11.475)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 8.625 10.825)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 8.625 9.325)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 8.625 7.825)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 8.625 6.325)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 8.625 4.825)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 8.625 3.325)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 8.625 1.825)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 8.625 0.325)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 8.625 -1.175)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 8.625 -2.675)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 8.625 -4.175)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 8.625 -5.675)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 8.625 -7.175)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 8.625 -8.775)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 8.625 -10.275)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 8.625 -11.675)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -1.19 -3.735)
		(size 4.1 4.1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -24 -13.023) (xy 24 -13.023) (xy 24 -34.323) (xy -24 -34.323)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-S2-WROVER.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
