(footprint "ESP32-S3-WROOM-2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2.4 GHz Wi­-Fi and Bluetooth 5 (LE) module: https://www.espressif.com/sites/default/files/documentation/esp32-s3-wroom-2_datasheet_en.pdf")
	(tags "Bluetooth WiFi Wi-Fi ESP WROOM")
	(property "Reference" "REF**"
		(at -10.5 13.5 90)
		(layer "F.SilkS")
	)
	(property "Value" "ESP32-S3-WROOM-2"
		(at 0 14.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 3 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -8.75 -5.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8.75 -3.99)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -8.75 -2.72)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -8.75 -1.45)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -8.75 -0.18)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -8.75 1.09)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.75 2.36)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8.75 3.63)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -8.75 4.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -8.75 6.17)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -8.75 7.44)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -8.75 8.71)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -8.75 9.98)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -8.75 11.25)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -6.985 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -5.715 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -4.445 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -3.175 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1.905 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -0.635 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0.635 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.905 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 3.175 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 4.445 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 5.715 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 6.985 12.5 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 8.75 11.25)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 8.75 9.98)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 8.75 8.71)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 8.75 7.44)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 8.75 6.17)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 8.75 4.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 8.75 3.63)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 8.75 2.36)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 8.75 1.09)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 8.75 -0.18)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 8.75 -1.45)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 8.75 -2.72)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 8.75 -3.99)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 8.75 -5.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -2.86 -1.41)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "41" thru_hole circle
		(at -2.86 -0.66)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at -2.86 0.09)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "41" thru_hole circle
		(at -2.86 0.84)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at -2.86 1.59)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "41" thru_hole circle
		(at -2.11 -1.41)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" thru_hole circle
		(at -2.11 0.09)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" thru_hole circle
		(at -2.11 1.59)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at -1.36 -1.41)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "41" thru_hole circle
		(at -1.36 -0.66)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at -1.36 0.09)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "41" thru_hole circle
		(at -1.36 0.84)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at -1.36 1.59)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "41" thru_hole circle
		(at -0.61 -1.41)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" thru_hole circle
		(at -0.61 0.09)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" thru_hole circle
		(at -0.61 1.59)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at 0.14 -1.41)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "41" thru_hole circle
		(at 0.14 -0.66)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at 0.14 0.09)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "41" thru_hole circle
		(at 0.14 0.84)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "41" smd rect
		(at 0.14 1.59)
		(size 1 1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -24 -27.75) (xy 24 -27.75) (xy 24 -6.75) (xy -24 -6.75)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-S3-WROOM-2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
