(footprint "ESP32-WROOM-32UE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2.4 GHz Wi-Fi and Bluetooth module, https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf")
	(tags "2.4 GHz Wi-Fi and Bluetooth module")
	(property "Reference" "REF**"
		(at 0 -10.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "ESP32-WROOM-32UE"
		(at 0 11.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -8.75 -8.41)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8.75 -7.14)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -8.75 -5.87)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -8.75 -4.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -8.75 -3.33)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -8.75 -2.06)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.75 -0.79)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8.75 0.48)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -8.75 1.75)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -8.75 3.02)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -8.75 4.29)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -8.75 5.56)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -8.75 6.83)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -8.75 8.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -5.715 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -4.445 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -3.175 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -1.905 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -0.635 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 0.635 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 1.905 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 3.175 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 4.445 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 5.715 9.35 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 8.75 8.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 8.75 6.83)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 8.75 5.56)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 8.75 4.29)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 8.75 3.02)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 8.75 1.75)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 8.75 0.48)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 8.75 -0.79)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 8.75 -2.06)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 8.75 -3.33)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 8.75 -4.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 8.75 -5.87)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 8.75 -7.14)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 8.75 -8.41)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -2.9 -2.47)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -2.9 -1.77)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" smd rect
		(at -2.9 -1.07)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -2.9 -0.37)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" smd rect
		(at -2.9 0.33)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -2.2 -2.47)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" thru_hole circle
		(at -2.2 -1.07)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" thru_hole circle
		(at -2.2 0.33)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" smd rect
		(at -1.5 -2.47)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -1.5 -1.77)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" smd rect
		(at -1.5 -1.07)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" smd rect
		(at -1.5 -1.07)
		(size 3.8 3.8)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "39" thru_hole circle
		(at -1.5 -0.37)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" smd rect
		(at -1.5 0.33)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -0.8 -2.47)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" thru_hole circle
		(at -0.8 -1.07)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" thru_hole circle
		(at -0.8 0.33)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" smd rect
		(at -0.1 -2.47)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -0.1 -1.77)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" smd rect
		(at -0.1 -1.07)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -0.1 -0.37)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "39" smd rect
		(at -0.1 0.33)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-WROOM-32UE.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
