(footprint "Garmin_M8-35_9.8x14.0mm_Layout6x6_P1.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "D52M ANT SoC Module https://www.thisisant.com/assets/resources/D00001687_D52_Module_Datasheet.v.2.3_(Garmin).pdf")
	(tags "RF SoC Radio ANT Bluetooth BLE D52 nRF52 Garmin Canada Dynastream Nordic")
	(property "Reference" "REF**"
		(at 0 8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Garmin_M8-35_9.8x14.0mm_Layout6x6_P1.5mm"
		(at 0 -8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.000001)
	(attr smd)
	(fp_text user "KEEP-OUT"
		(at 0 -4.4 0)
		(layer "Cmts.User")
	)
	(fp_text user "COPPER"
		(at 0 -6.1 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A2" smd circle
		(at -2.25 -1.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A3" smd circle
		(at -0.75 -1.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0.75 -1.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A5" smd circle
		(at 2.25 -1.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A6" smd circle
		(at 3.75 -1.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B1" smd circle
		(at -3.75 -0.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" smd circle
		(at -2.25 -0.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B3" smd circle
		(at -0.75 -0.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0.75 -0.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B5" smd circle
		(at 2.25 -0.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B6" smd circle
		(at 3.75 -0.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C1" smd circle
		(at -3.75 1.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C2" smd circle
		(at -2.25 1.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C3" smd circle
		(at -0.75 1.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0.75 1.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C5" smd circle
		(at 2.25 1.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C6" smd circle
		(at 3.75 1.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D1" smd circle
		(at -3.75 2.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D2" smd circle
		(at -2.25 2.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D3" smd circle
		(at -0.75 2.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0.75 2.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D5" smd circle
		(at 2.25 2.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D6" smd circle
		(at 3.75 2.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "E1" smd circle
		(at -3.75 4.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "E2" smd circle
		(at -2.25 4.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "E3" smd circle
		(at -0.75 4.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "E4" smd circle
		(at 0.75 4.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "E5" smd circle
		(at 2.25 4.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "E6" smd circle
		(at 3.75 4.25)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "F1" smd circle
		(at -3.75 5.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "F2" smd circle
		(at -2.25 5.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "F3" smd circle
		(at -0.75 5.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "F4" smd circle
		(at 0.75 5.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "F5" smd circle
		(at 2.25 5.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(pad "F6" smd circle
		(at 3.75 5.75)
		(size 0.762 0.762)
		(layers "F.Cu" "F.Mask")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -4.9 -2.6) (xy 4.9 -2.6) (xy 4.9 -7) (xy -4.9 -7)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Garmin_M8-35_9.8x14.0mm_Layout6x6_P1.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
