(footprint "IQRF_TRx2DA_KON-SIM-01"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8 pin SIM connector for IQRF TR-x2DA(T) modules, http://iqrf.org/weben/downloads.php?id=104")
	(tags "IQRF_KON-SIM-01 IQRF_TRx2DA")
	(property "Reference" "REF**"
		(at 0.1 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "IQRF_TRx2DA_KON-SIM-01"
		(at 0 24 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Antenna"
		(at 0 20 0)
		(layer "Cmts.User")
	)
	(fp_text user "KEEP OUT ZONE"
		(at 0 14.75 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -7.075 -1.07)
		(size 1.7 4.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 7.075 -1.07)
		(size 1.7 4.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd rect
		(at -3.895 -4.975)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd rect
		(at -1.355 -4.975)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd rect
		(at 1.185 -4.975)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd rect
		(at 3.725 -4.975)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd rect
		(at -3.895 4.975)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd rect
		(at -1.355 4.975)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd rect
		(at 1.185 4.975)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd rect
		(at 3.725 4.975)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -8.5 11.75) (xy 8.5 11.75) (xy 8.5 22.75) (xy -8.5 22.75)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/IQRF_TRx2DA_KON-SIM-01.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
