(footprint "Jadak_Thingmagic_M6e-Nano"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "UHF RFID reader with one 27dBm antenna port, https://www.jadaktech.com/product/thingmagic-m6e-nano-uhf-rain-rfid/")
	(tags "Jadak Thingmagic M6e")
	(property "Reference" "REF**"
		(at -9.3 -14 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jadak_Thingmagic_M6e-Nano"
		(at 0 14.4 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -2.8 -10.95)
		(size 4.2 2.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.95 -8.3)
		(size 11.7 1.6)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1 -2.7)
		(size 3 3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1 1.1)
		(size 3 3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.9 -2.7)
		(size 3 3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.9 1.1)
		(size 3 3)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -10.78 -11 180)
		(size 2.365 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -10.78 -9.75 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -10.78 -8.5 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -10.78 -7.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -10.78 -6 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -10.78 -4.75 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -10.78 -3.5 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -10.78 -2.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -10.78 -1 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -10.78 0.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -10.78 1.5 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -10.78 2.75 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -10.78 4 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -10.78 5.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -10.78 6.5 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -10.78 7.75 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -10.78 9 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -10.78 10.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 10.78 10.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 10.78 9 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 10.78 7.75 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 10.78 6.5 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 10.78 5.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 10.78 4 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 10.78 2.75 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 10.78 1.5 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 10.78 0.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 10.78 -1 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 10.78 -2.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 10.78 -3.5 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 10.78 -4.75 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 10.78 -6 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 10.78 -7.25 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 10.78 -8.5 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 10.78 -9.75 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 10.78 -11 180)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 7.5 -13.22 90)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 6.25 -13.22 90)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 5 -13.22 90)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 3.75 -13.22 90)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" thru_hole circle
		(at -4.6 -11.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -4.6 -9.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -4.6 -7.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -3.7 -10.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -3.7 -8.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -2.8 -11.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -2.8 -9.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" smd roundrect
		(at -2.8 -9.8)
		(size 4.6 5)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.05434782609)
	)
	(pad "41" thru_hole circle
		(at -2.8 -7.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -1.9 -10.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -1.9 -8.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -1 -11.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -1 -9.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -1 -7.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -0.1 -8.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.25 -3.5)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.25 -2.15)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.25 -0.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.25 0.55)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.25 1.9)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 0.8 -7.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.6 -3.5)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.6 -2.15)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.6 -0.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.6 0.55)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.6 1.9)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 1.7 -8.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" smd roundrect
		(at 2.5 -13.22 90)
		(size 2.368 0.853)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" thru_hole circle
		(at 2.6 -7.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 2.95 -3.5)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 2.95 -2.15)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 2.95 -0.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" smd roundrect
		(at 2.95 -0.8)
		(size 7.3 7.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.03472222222)
	)
	(pad "41" thru_hole circle
		(at 2.95 0.55)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 2.95 1.9)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" smd roundrect
		(at 3.25 -8.3)
		(size 8 2)
		(drill
			(offset -0.25 0)
		)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "41" thru_hole circle
		(at 3.5 -8.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 4.3 -3.5)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 4.3 -2.15)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 4.3 -0.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 4.3 0.55)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 4.3 1.9)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 4.4 -7.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 5.3 -8.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 5.65 -3.5)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 5.65 -2.15)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 5.65 -0.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 5.65 0.55)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 5.65 1.9)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 6.2 -7.8)
		(size 0.8 0.8)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -9.2 -11.9) (xy -5.1 -11.9) (xy -5.1 -4.4) (xy -0.7 -4.4) (xy -0.7 2.8) (xy 9.2 2.8) (xy 9.2 12.3)
				(xy -9.2 12.3)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.5 -11.9) (xy 9.2 -11.9) (xy 9.2 2.8) (xy 6.6 2.8) (xy 6.6 -4.4) (xy -5.1 -4.4) (xy -5.1 -7.3)
				(xy 7 -7.3) (xy 7 -9.3) (xy -0.5 -9.3)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Jadak_Thingmagic_M6e-Nano.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
