(footprint "MCU_Seeed_ESP32C3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ESP32C3 Seeed Xiao RF Wifi Shield (https://www.seeedstudio.com/blog/wp-content/uploads/2022/08/Seeed-Studio-XIAO-Series-Package-and-PCB-Design.pdf)")
	(tags "wifi bluetooth microcontroller")
	(property "Reference" "REF**"
		(at 7 -12 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "MCU_Seeed_ESP32C3"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 1.1 -0.4)
		(size 1.5 1.5)
		(property pad_prop_heatsink)
		(layers "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "" smd roundrect
		(at 1.1 1.6)
		(size 1.5 1.5)
		(property pad_prop_heatsink)
		(layers "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "" smd roundrect
		(at 3.1 -0.4)
		(size 1.5 1.5)
		(property pad_prop_heatsink)
		(layers "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "" smd roundrect
		(at 3.1 1.6)
		(size 1.5 1.5)
		(property pad_prop_heatsink)
		(layers "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "1" smd roundrect
		(at -8.5 -7.62)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -8.5 -5.08)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -8.5 -2.54)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -8.5 0)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -8.5 2.54)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at -8.5 5.08)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at -8.5 7.62)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 8.5 7.62)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at 8.5 5.08)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 8.5 2.54)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at 8.5 0)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at 8.5 -2.54)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at 8.5 -5.08)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at 8.5 -7.62)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at 2.1 0.6)
		(size 3.5 3.5)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.07142857143)
	)
	(pad "16" smd roundrect
		(at -4.5 -0.4)
		(size 2.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1923076923)
	)
	(pad "17" smd roundrect
		(at -4.5 -2.3)
		(size 2.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1923076923)
	)
	(pad "18" smd circle
		(at -1.27 -8.62)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd circle
		(at -1.27 -6.04)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd circle
		(at -1.27 -3.5)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd circle
		(at 1.27 -3.5)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd circle
		(at 1.27 -6.04)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd circle
		(at 1.27 -8.62)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/MCU_Seeed_ESP32C3.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
