(footprint "Microchip_BM83"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Microchip BM83, Bluetooth 5.0 Stereo Audio Module with on-Board antenna, https://ww1.microchip.com/downloads/aemDocuments/documents/WSG/ProductDocuments/DataSheets/70005402E.pdf")
	(tags "bluetooth module")
	(property "Reference" "REF**"
		(at 7.73 17.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Microchip_BM83"
		(at 0 17 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "TEST"
		(at 4 -4.9 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Antenna area"
		(at -0.4 -10 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -7.25 -4.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -7.25 -3.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -7.25 -2.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -7.25 -1.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -7.25 -0.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at -7.25 0.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at -7.25 1.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at -7.25 2.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at -7.25 3.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at -7.25 4.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at -7.25 5.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at -7.25 6.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at -7.25 7.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at -7.25 8.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at -7.25 9.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd roundrect
		(at -7.25 10.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd roundrect
		(at -7.25 11.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd roundrect
		(at -7.25 12.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "19" smd roundrect
		(at -7.25 13.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "20" smd roundrect
		(at -7.25 14.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "21" smd roundrect
		(at -4.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "22" smd roundrect
		(at -3.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "23" smd roundrect
		(at -2.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "24" smd roundrect
		(at -1.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "25" smd roundrect
		(at -0.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "26" smd roundrect
		(at 0.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "27" smd roundrect
		(at 1.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "28" smd roundrect
		(at 2.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "29" smd roundrect
		(at 3.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "30" smd roundrect
		(at 4.5 15.75)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "31" smd roundrect
		(at 7.25 14.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "32" smd roundrect
		(at 7.25 13.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "33" smd roundrect
		(at 7.25 12.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "34" smd roundrect
		(at 7.25 11.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "35" smd roundrect
		(at 7.25 10.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "36" smd roundrect
		(at 7.25 9.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "37" smd roundrect
		(at 7.25 8.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "38" smd roundrect
		(at 7.25 7.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "39" smd roundrect
		(at 7.25 6.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "40" smd roundrect
		(at 7.25 5.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "41" smd roundrect
		(at 7.25 4.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "42" smd roundrect
		(at 7.25 3.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "43" smd roundrect
		(at 7.25 2.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "44" smd roundrect
		(at 7.25 1.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "45" smd roundrect
		(at 7.25 0.1)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "46" smd roundrect
		(at 7.25 -0.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "47" smd roundrect
		(at 7.25 -1.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "48" smd roundrect
		(at 7.25 -2.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "49" smd roundrect
		(at 7.25 -3.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "50" smd roundrect
		(at 7.25 -4.9)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "56" smd roundrect
		(at 4.77 5.53)
		(size 1.78 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1404494382)
		(thermal_bridge_angle 45)
	)
	(pad "57" smd roundrect
		(at -3.29 -4.58)
		(size 2.79 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -6.3 -6) (xy -6.3 14.6) (xy -7.5 14.6) (xy -7.5 16) (xy -5 16) (xy -5 14.8) (xy 5 14.8) (xy 5 16)
				(xy 7.5 16) (xy 7.5 14.6) (xy 6.3 14.6) (xy 6.3 -6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "Cmts.User" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu"
			"In14.Cu" "In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu"
			"In21.Cu" "In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu"
			"In28.Cu" "In29.Cu" "In30.Cu"
		)
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -22.5 -31) (xy -22.5 -6) (xy 22.5 -6) (xy 22.5 -31)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Microchip_BM83.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
