(footprint "MonoWireless_TWE-L-WX"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.mono-wireless.com/jp/products/TWE-LITE/MW-PDS-TWELITE-JP.pdf")
	(tags "TWE-L-WX")
	(property "Reference" "REF**"
		(at 0 -8.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "MonoWireless_TWE-L-WX"
		(at 0 8.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -0.8 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole oval
		(at -3.7 -3.9 315)
		(size 4.3 3.1)
		(drill oval 4.3 3.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd oval
		(at -6.735 -4.445 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -6.735 -3.175 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -6.735 -1.905 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -6.735 -0.635 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -6.735 0.635 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -6.735 1.905 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -6.735 3.175 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -6.735 4.445 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -4.445 6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -3.175 6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -1.905 6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -0.635 6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at 0.635 6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 1.905 6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at 3.175 6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at 4.445 6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at 6.735 4.445 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at 6.735 3.175 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at 6.735 1.905 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at 6.735 0.635 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at 6.735 -0.635 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at 6.735 -1.905 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at 6.735 -3.175 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at 6.735 -4.445 90)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at 4.445 -6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 3.175 -6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 1.905 -6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 0.635 -6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at -0.635 -6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at -1.905 -6.735)
		(size 0.9 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at -3.175 -6.835)
		(size 0.9 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at -4.445 -6.835)
		(size 0.9 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/MonoWireless_TWE-L-WX.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
