(footprint "NINA-B111"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "NINA-B111 LGA module 42 Pin https://content.u-blox.com/sites/default/files/NINA-B1_DataSheet_UBX-15019243.pdf#page=30")
	(tags "NINA ublox u-blox b111 bluetooth nrf52840 module")
	(property "Reference" "REF**"
		(at -3.3 -6.9 180)
		(layer "F.SilkS")
	)
	(property "Value" "NINA-B111"
		(at 0 6.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Please check the datasheet."
		(at 0 3.65 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Depanelization residues area"
		(at 5.2 0 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Pins 6,12,14,26,30 might need"
		(at 0 2.4 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "soldermask adjustments."
		(at 0 3.05 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.125 -4.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd roundrect
		(at -4.125 -3.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "3" smd roundrect
		(at -4.125 -2.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "4" smd roundrect
		(at -4.125 -1.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "5" smd roundrect
		(at -4.125 -0.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "6" smd roundrect
		(at -4.125 0.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "7" smd roundrect
		(at -4.125 1.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "8" smd roundrect
		(at -4.125 2.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "9" smd roundrect
		(at -4.125 3.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "10" smd roundrect
		(at -4.125 4.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "11" smd roundrect
		(at -2 4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "12" smd roundrect
		(at -1 4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "13" smd roundrect
		(at 0 4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "14" smd roundrect
		(at 1 4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "15" smd roundrect
		(at 2 4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "16" smd roundrect
		(at 4.125 4.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "17" smd roundrect
		(at 4.125 3.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "18" smd roundrect
		(at 4.125 2.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "19" smd roundrect
		(at 4.125 1.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "20" smd roundrect
		(at 4.125 0.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "21" smd roundrect
		(at 4.125 -0.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "22" smd roundrect
		(at 4.125 -1.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "23" smd roundrect
		(at 4.125 -2.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "24" smd roundrect
		(at 4.125 -3.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "25" smd roundrect
		(at 4.125 -4.5)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "26" smd roundrect
		(at 2 -4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "27" smd roundrect
		(at 1 -4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "28" smd roundrect
		(at 0 -4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "29" smd roundrect
		(at -1 -4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "30" smd roundrect
		(at -2 -4.425 90)
		(size 1.15 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "31" smd roundrect
		(at -0.575 -1.725 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "32" smd roundrect
		(at 0.575 -1.725 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "33" smd roundrect
		(at -1.725 -0.575 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "34" smd roundrect
		(at -0.575 -0.575 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "35" smd roundrect
		(at 0.575 -0.575 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "36" smd roundrect
		(at 1.725 -0.575 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "37" smd roundrect
		(at -0.575 0.575 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "38" smd roundrect
		(at 0.575 0.575 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "39" smd roundrect
		(at -1.725 1.725 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "40" smd roundrect
		(at -0.575 1.725 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "41" smd roundrect
		(at 0.575 1.725 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "42" smd roundrect
		(at 1.725 1.725 270)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "Depanelization residues area")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 5.35 5.3) (xy 5 5.3) (xy 5 -5.3) (xy 5.35 -5.3)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/NINA-B111.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
