(footprint "Particle_P1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://docs.particle.io/datasheets/p1-datasheet/")
	(tags "Particle P1")
	(property "Reference" "REF**"
		(at -8.09 14.84 180)
		(layer "F.SilkS")
	)
	(property "Value" "Particle_P1"
		(at 0 1.21 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "No metal, traces or"
		(at 0 -8.92 0)
		(layer "Cmts.User")
	)
	(fp_text user "components on any layer"
		(at 0 -7.6 0)
		(layer "Cmts.User")
	)
	(fp_text user "KEEP-OUT ZONE"
		(at 0 -11.34 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -9.4 -1.64 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -9.4 -0.64 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -9.4 0.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -9.4 1.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -9.4 2.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -9.4 3.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -9.4 4.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -9.4 5.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -9.4 6.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -9.4 7.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -9.4 8.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -9.4 9.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -9.4 10.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -9.4 11.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -9.4 12.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -8 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -7 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -6 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -5 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -4 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -3 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -2 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -1 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 1 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 2 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 3 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 4 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 5 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 6 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 7 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 8 13.26 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 9.4 12.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 9.4 11.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 9.4 10.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 9.4 9.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 9.4 8.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 9.4 7.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 9.4 6.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 9.4 5.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 9.4 4.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 9.4 3.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 9.4 2.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 9.4 1.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 9.4 0.36 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 9.4 -0.64 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 9.4 -1.64 270)
		(size 0.6 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 8 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 7 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 6 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 5 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 4 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 3 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 2 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 1 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 0 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -1 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -2 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -3 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at -4 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at -5 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at -6 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at -7 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at -8 -2.44 270)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at -3.5 2.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at -3.5 5.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at -3.5 8.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at 0 2.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at 0 5.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at 0 8.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at 3.5 2.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at 3.5 5.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at 3.5 8.63 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at 9.12 -13.26 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at -9.12 -13.26 270)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -7.695372 -1.14) (xy -7.713743 -1.244189) (xy -7.766641 -1.335811) (xy -7.847686 -1.403816)
				(xy -7.947102 -1.44) (xy -8.052898 -1.44) (xy -8.152314 -1.403816) (xy -8.233359 -1.335811) (xy -8.286257 -1.244189)
				(xy -8.304628 -1.14) (xy -8.286257 -1.035811) (xy -8.233359 -0.944189) (xy -8.152314 -0.876184)
				(xy -8.052898 -0.84) (xy -7.947102 -0.84) (xy -7.847686 -0.876184) (xy -7.766641 -0.944189) (xy -7.713743 -1.035811)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -10 -12.66) (xy -10 -3.04) (xy 10 -3.04) (xy 10 -12.66) (xy 8.52 -12.66) (xy 8.52 -14.14) (xy -8.52 -14.14)
				(xy -8.52 -12.66)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Particle_P1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
