(footprint "RN42N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Class 2 Bluetooth Module without antenna")
	(tags "Bluetooth Module")
	(property "Reference" "REF**"
		(at 6.858 11.176 0)
		(layer "F.SilkS")
	)
	(property "Value" "RN42N"
		(at 0.3 0 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.03 -1.65 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -6.4 -6)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -6.4 -4.8)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -6.4 -3.6)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -6.4 -2.4)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -6.4 -1.2)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -6.4 0)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -6.4 1.2)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -6.4 2.4)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -6.4 3.6)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -6.4 4.8)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -6.4 6)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -6.4 7.2)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at 6.4 7.2)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 6.4 6)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at 6.4 4.8)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at 6.4 3.6)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at 6.4 2.4)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at 6.4 1.2)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at 6.4 0)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at 6.4 -1.2)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at 6.4 -2.4)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at 6.4 -3.6)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at 6.4 -4.8)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at 6.4 -6)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at 3.8 -9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 2.2 -9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 0.6 -9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 3.1 9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at -3.1 9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 4.1 9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 1.8 9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 0.6 9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at -0.6 9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at -1.8 9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at -4.1 9.7 90)
		(size 2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -5.6 -9.7)
		(size 1.8 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -5.6 9.3)
		(size 1.8 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 5.6 -9.7)
		(size 1.8 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 5.6 9.3)
		(size 1.8 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/RN42N.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
