(footprint "Raytac_MDBT50Q"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Multiprotocol radio SoC module https://www.raytac.com/download/index.php?index_id=43")
	(tags "wireless 2.4 GHz Bluetooth ble zigbee 802.15.4 thread nordic raytac nrf52840 nrf52833")
	(property "Reference" "REF**"
		(at -6 0 270)
		(layer "F.SilkS")
	)
	(property "Value" "Raytac_MDBT50Q"
		(at 0.2 8.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "TOP LAYER"
		(at -1.6 -3.6 0)
		(layer "Cmts.User")
	)
	(fp_text user "KEEP OUT"
		(at -1.5 -3.1 0)
		(layer "Cmts.User")
	)
	(fp_text user "KEEP OUT ZONE"
		(at 0.05 -5.75 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.05 1.75 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.65 -3.75)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.65 -2.65)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.65 -1.85)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.65 -0.25)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.75 0.15)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.65 0.55)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.75 0.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.65 1.35)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.75 1.75)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -4.65 2.15)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.75 2.55)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -4.65 2.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.75 3.35)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -4.65 3.75)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -4.8 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -4 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -3.2 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -2.4 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -2 6.25 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -1.6 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.2 6.25 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -0.8 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -0.4 6.25 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 0.4 6.25 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 0.8 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 1.2 6.25 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 1.6 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 2 6.25 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 2.4 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 3.2 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 4 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 4.8 7.15 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 4.65 6.15)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 4.65 5.35)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.75 4.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 4.65 4.55)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 3.75 4.15)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 4.65 3.75)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 3.75 3.35)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 4.65 2.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 3.75 2.55)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 3.75 1.75)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 4.65 1.35)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 3.75 0.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 4.65 0.55)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 3.75 0.15)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 4.65 -0.25)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 3.75 -0.65)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 3.75 -1.45)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 4.65 -1.85)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 3.75 -2.25)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 4.65 -2.65)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 3.75 -3.05)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 4.65 -3.75)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -2 0.55 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -1.2 0.55 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -0.4 0.55 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at 0.4 0.55 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at 1.2 0.55 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at 2 0.55 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -0.7 -2.75) (xy -2.3 -2.75) (xy -2.3 -3.95) (xy -0.7 -3.95)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -6.2 -4) (xy 6.2 -4) (xy 6.2 -7.75) (xy -6.2 -7.75)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Raytac_MDBT50Q.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
