(footprint "ST-SiP-LGA-86-11x7.3mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "STM32WB5MMG  Module, LGA86L 11x7.3")
	(tags "bluetooth bluetooth5 bluetooth5.0 802.15.4 zigbee thread module stm32 rf")
	(property "Reference" "REF**"
		(at 0 -6.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST-SiP-LGA-86-11x7.3mm"
		(at -0.15 6.565 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 270)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.175 -2.075)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.175 -1.6)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.175 -1.15)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.175 -0.7)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.175 -0.25)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.175 0.2)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.175 0.65)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.175 1.1)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.175 1.55)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -3.175 2)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.175 2.45)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.175 2.9)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.175 3.35)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -3.175 3.8)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -3.175 4.25)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3.175 4.7)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -3.175 5.175)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -2.7 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -2.25 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -1.8 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.35 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -0.9 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -0.45 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 0.45 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 0.9 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 1.35 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 1.8 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 2.25 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 2.7 5.175)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 3.175 5.175)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 3.175 4.7)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 3.175 4.25)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.175 3.8)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 3.175 3.35)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.175 2.9)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 3.175 2.45)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 3.175 2)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 3.175 1.55)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 3.175 1.1)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 3.175 0.65)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 3.175 0.2)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 3.175 -0.25)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 3.175 -0.7)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 3.175 -1.15)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 3.175 -1.6)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 3.175 -2.075)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 2.7 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 2.25 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 1.8 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 1.35 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 0.9 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 0.45 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 0 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -0.45 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -0.9 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -1.35 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -1.8 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -2.25 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at -2.7 -2.075)
		(size 0.3 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at -1.35 -0.7)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at -1.35 0.2)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at -1.35 1.1)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at -1.35 2)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at -1.35 2.9)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at -1.35 3.8)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at -0.45 3.8)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at 0.45 3.8)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at 1.35 3.8)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at 1.35 2.9)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at 1.35 2)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at 1.35 1.1)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at 1.35 0.2)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at 1.35 -0.7)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at 0.45 -0.7)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at -0.45 -0.7)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at -0.45 0.2)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at -0.45 1.1)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at -0.45 2)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at -0.45 2.9)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at 0.45 2.9)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at 0.45 2)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at 0.45 1.1)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at 0.45 0.2)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at -3.05 -5.035)
		(size 0.43 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at 3.05 -5.035)
		(size 0.43 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 2.65 -3) (xy -4.95 -3) (xy -4.95 -6.5) (xy 2.65 -6.5)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ST-SiP-LGA-86-11x7.3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
