(footprint "ST_SPBTLE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Bluetooth Low Energy Module")
	(tags "ble module st bluetooth")
	(property "Reference" "REF**"
		(at 4.55 -9.61 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_SPBTLE"
		(at 3 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "on any layer"
		(at -4 -11 0)
		(layer "Cmts.User")
	)
	(fp_text user "No copper"
		(at -3.95 -12.11 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.86 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.75 -3.19)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.75 -1.92)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.75 -0.65)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -6.75 0.62)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -6.75 1.89)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.75 2.89 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 6.75 1.89)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 6.75 0.62)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 6.75 -0.65)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 6.75 -1.92)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.75 -3.19)
		(size 1.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 2.05 -1.11) (xy -5.95 -1.1) (xy -5.95 -3.7) (xy -7.55 -3.7) (xy -9.95 -3.7) (xy -9.95 -13.11)
				(xy 2.05 -13.11)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ST_SPBTLE.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
