(footprint "Taiyo-Yuden_EYSGJNZWY"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Taiyo Yuden NRF51822 Module Bluetooth https://www.yuden.co.jp/wireless_module/document/datareport2/en/TY_BLE_EYSGJNZ_DataReport_V1_9_20180530E.pdf")
	(tags "Taiyo Yuden NRF51822 Module Bluetooth ")
	(property "Reference" "REF**"
		(at 0 -6.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Taiyo-Yuden_EYSGJNZWY"
		(at 0 6.7 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEP OUT ZONE"
		(at 0 4.25 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at 0 -2)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -0.5)
		(size 1.2 1.1)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.075 -5.05)
		(size 0.55 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.035)
	)
	(pad "2" smd rect
		(at -1.95 -4.05)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "3" smd rect
		(at -1.95 -3.25)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "4" smd rect
		(at -1.95 -2.45)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "5" smd rect
		(at -1.95 -1.65)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "6" smd rect
		(at -1.95 -0.85)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "7" smd rect
		(at -1.95 -0.05)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "8" smd rect
		(at -1.95 0.75)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "9" smd rect
		(at -1.95 1.625)
		(size 0.8 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.035)
	)
	(pad "10" smd rect
		(at -0.4 1.35)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "11" smd rect
		(at 0.4 1.35)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "12" smd rect
		(at 1.95 1.625)
		(size 0.8 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.035)
	)
	(pad "13" smd rect
		(at 1.95 0.75)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "14" smd rect
		(at 1.95 -0.05)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "15" smd rect
		(at 1.95 -0.85)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "16" smd rect
		(at 1.95 -1.65)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "17" smd rect
		(at 1.95 -2.45)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "18" smd rect
		(at 1.95 -3.25)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "19" smd rect
		(at 1.95 -4.05)
		(size 0.8 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "20" smd rect
		(at 2.075 -5.05)
		(size 0.55 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.035)
	)
	(pad "21" smd rect
		(at 1.2 -5.05)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "22" smd rect
		(at 0.4 -5.05)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "23" smd rect
		(at -0.4 -5.05)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "24" smd rect
		(at -1.2 -5.05)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "25" smd rect
		(at 0.8 -3.85)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "26" smd rect
		(at 0 -3.85)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "27" smd rect
		(at -0.8 -3.85)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.03)
	)
	(pad "28" smd rect
		(at 0 -1.25)
		(size 1.5 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -7.55 2.9) (xy 7.55 2.9) (xy 7.55 5.65) (xy -7.55 5.65)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Taiyo-Yuden_EYSGJNZWY.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
