(footprint "Laird_Technologies_97-2003_12.70x13.37mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Laird Technologies 97-2003 EZ PEEL Shielding Cabinet One Piece SMD 12.70x13.37mm (https://assets.lairdtech.com/home/brandworld/files/Board%20Level%20Shields%20Catalog%20Download.pdf)")
	(tags "Shielding Cabinet")
	(property "Reference" "REF**"
		(at 0 -7.96 0)
		(layer "F.SilkS")
	)
	(property "Value" "Laird_Technologies_97-2003_12.70x13.37mm"
		(at 0 7.96 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.285 -6.77)
		(size 0.38 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -6.285 0)
		(size 0.38 13.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -6.285 6.77)
		(size 0.38 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 0 -6.77)
		(size 12.19 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 0 6.77)
		(size 12.19 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 6.285 -6.77)
		(size 0.38 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 6.285 0)
		(size 0.38 13.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 6.285 6.77)
		(size 0.38 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Shielding.3dshapes/Laird_Technologies_97-2003_12.70x13.37mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
