(footprint "USR-C322"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.usriot.com/download/WIFI/USR-C322-Hardware-Manual_V1.2.01.pdf")
	(tags "WiFi IEEE802.11 b/g/n")
	(property "Reference" "REF**"
		(at -8.34 11.955 0)
		(layer "F.SilkS")
	)
	(property "Value" "USR-C322"
		(at 0.43 0.745 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Antenna"
		(at 0.63 -17.265 0)
		(layer "Cmts.User")
	)
	(fp_text user "No Copper"
		(at 0.7 -14.435 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.32 -1.265 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -9.31 -10.385)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -9.31 -9.115)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -9.31 -7.845)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -9.31 -6.575)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -9.31 -5.305)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -9.31 -4.035)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -9.31 -2.765)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -9.31 -1.495)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -9.31 -0.225)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -9.31 1.045)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -9.31 2.315)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -9.31 3.585)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -9.31 4.855)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -9.31 6.125)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -9.31 7.395)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -9.31 8.665)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -6.96 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -5.69 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -4.42 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -3.15 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.88 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -0.61 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 0.66 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 1.93 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 3.2 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 4.47 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 5.74 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 7.01 10.135 90)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 9.31 8.665)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 9.31 7.395)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 9.31 6.125)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 9.31 4.855)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 9.31 3.585)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 9.31 2.315)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 9.31 1.045)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 9.31 -0.225)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 9.31 -1.495)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 9.31 -2.765)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 9.31 -4.035)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 9.31 -5.305)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 9.31 -6.575)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 9.31 -7.845)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 9.31 -9.115)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 9.31 -10.385)
		(size 1.4 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_WiFi.3dshapes/USR-C322.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
