(footprint "Relay_2P2T_10x6mm_TE_IMxxG"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Signal Relay, 10x6mm, 2 Form C, Gull Wings, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7F108-98001%7FZ.1%7Fpdf%7FEnglish%7FENG_DS_108-98001_Z.1.pdf")
	(tags "TE IM-Series Relay DPDT Form C")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_2P2T_10x6mm_TE_IMxxG"
		(at 0 6.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.06 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3 -3.8)
		(size 2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3 -0.6)
		(size 2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3 1.6)
		(size 2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3 3.8)
		(size 2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 3 3.8)
		(size 2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3 1.6)
		(size 2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3 -0.6)
		(size 2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3 -3.8)
		(size 2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_SMD.3dshapes/Relay_2P2T_10x6mm_TE_IMxxG.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
