(footprint "Relay_DPDT_Kemet_EE2_NUX_DoubleCoil"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Kemet signal relay, DPDT, double coil latching, https://content.kemet.com/datasheets/KEM_R7002_EC2_EE2.pdf")
	(tags "Kemet EC2 signal relay DPDT double dual coil latching surface mount SMD")
	(property "Reference" "REF**"
		(at 0 -9 180)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_DPDT_Kemet_EE2_NUX_DoubleCoil"
		(at -6.06 -0.06 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.01 0.39 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.51 -6.35 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "3" smd roundrect
		(at -3.51 -1.27 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "4" smd roundrect
		(at -3.51 1.27 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "5" smd roundrect
		(at -3.51 3.81 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "6" smd roundrect
		(at -3.51 6.35 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "7" smd roundrect
		(at 3.51 6.35 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "8" smd roundrect
		(at 3.51 3.81 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "9" smd roundrect
		(at 3.51 1.27 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "10" smd roundrect
		(at 3.51 -1.27 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(pad "12" smd roundrect
		(at 3.51 -6.35 270)
		(size 1.11 2.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.225)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_SMD.3dshapes/Relay_DPDT_Kemet_EE2_NUX_DoubleCoil.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
