(footprint "Relay_DPDT_Omron_G6K-2G"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Omron G6K-2G relay package http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf")
	(tags "Omron G6K-2G relay")
	(property "Reference" "REF**"
		(at 0.16 -6.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_DPDT_Omron_G6K-2G"
		(at -0.04 6.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.01 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.85 -3.8)
		(size 1.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.85 -1.27)
		(size 1.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.85 1.27)
		(size 1.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.85 3.81)
		(size 1.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.85 3.81)
		(size 1.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.85 1.27)
		(size 1.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.85 -1.27)
		(size 1.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.85 -3.81)
		(size 1.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_SMD.3dshapes/Relay_DPDT_Omron_G6K-2G.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
