(footprint "Relay_1-Form-B_Schrack-RYII_RM5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay, 1-Form-B, Schrack-RYII, RM5mm, SPST-NC")
	(tags "Relay 1-Form-B Schrack-RYII RM5mm SPST-NC")
	(property "Reference" "REF**"
		(at 10.9 -10.12 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_1-Form-B_Schrack-RYII_RM5mm"
		(at 10.9 2.58 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11 -3.8 0)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 18.9 0)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 23.94 -7.62)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole rect
		(at 0 0)
		(size 2.54 2.54)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A2" thru_hole circle
		(at 0 -7.62)
		(size 2.54 2.54)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_1-Form-B_Schrack-RYII_RM5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
