(footprint "Relay_3PST_COTO_3650"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Low thermal EMF 3PST-NO reed relay, 150V 0.25A, similar to 3660 but with independent shield, https://cotorelay.com/wp-content/uploads/2014/09/3600_series_reed_relay_datasheet.pdf")
	(tags "reed relay low thermal emf")
	(property "Reference" "REF**"
		(at 12.7 -4.445 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_3PST_COTO_3650"
		(at 12.7 4.445 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12.7 5.715 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "13" thru_hole circle
		(at 0 2.54 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 25.4 2.54 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 0 5.08 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 25.4 5.08 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 0 7.62 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 25.4 7.62 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole rect
		(at 0 0 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A2" thru_hole circle
		(at 25.4 0 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 0 10.16 90)
		(size 1.36 1.36)
		(drill 0.86)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_3PST_COTO_3650.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
