(footprint "Relay_DPDT_Finder_40.52"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DPDT relay, Finder 40.52, 8A, 250V, body size 29x12.4mm, height 25mm, pitch 5x7.5mm, https://cdn.findernet.com/app/uploads/S40EN.pdf")
	(tags "2-Form-C")
	(property "Reference" "REF**"
		(at 12 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_DPDT_Finder_40.52"
		(at 12 11.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12 3.75 0)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 20 0)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 15 0)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 25 0)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 20 7.5)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 15 7.5)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 25 7.5)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.08928571429)
	)
	(pad "A2" thru_hole circle
		(at 0 7.5)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Finder_40.52.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
