(footprint "Relay_DPDT_Fujitsu_FTR-F1C"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.fujitsu.com/downloads/MICRO/fcai/relays/ftr-f1.pdf")
	(tags "relay dpdt fujitsu tht")
	(property "Reference" "REF**"
		(at 4.15 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_DPDT_Fujitsu_FTR-F1C"
		(at 2.119657 13.5 270)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.5 13.2 270)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 270)
		(size 2.5 2.5)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 5 270)
		(size 2.5 2.5)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 10 270)
		(size 2.5 2.5)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 25 270)
		(size 2.5 2.5)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 7.5 25 270)
		(size 2.5 2.5)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 7.5 10 270)
		(size 2.5 2.5)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 7.5 5 270)
		(size 2.5 2.5)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 7.5 0 270)
		(size 2.5 2.5)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Fujitsu_FTR-F1C.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
