(footprint "Relay_DPDT_Schrack-RT2-FormC-Dual-Coil_RM5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay DPDT Schrack-RT2 RM5mm 16A 250V AC Form C http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FRT2_bistable%7F1116%7Fpdf%7FEnglish%7FENG_DS_RT2_bistable_1116.pdf%7F1-1415537-8")
	(tags "Relay DPDT Schrack-RT2 RM5mm 16A 250V AC Relay")
	(property "Reference" "REF**"
		(at 12.5 -11.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_DPDT_Schrack-RT2-FormC-Dual-Coil_RM5mm"
		(at 12.192 4.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12.065 -3.81 180)
		(layer "F.Fab")
	)
	(pad "11" thru_hole oval
		(at 20.3 0 180)
		(size 2 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 15.26 0 180)
		(size 2 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 25.34 0 180)
		(size 2 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole oval
		(at 20.3 -7.5 180)
		(size 2 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 15.26 -7.5 180)
		(size 2 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole oval
		(at 25.34 -7.5 180)
		(size 2 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole rect
		(at 0 0 180)
		(size 3 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A2" thru_hole oval
		(at 0 -7.5 180)
		(size 3 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A3" thru_hole oval
		(at 0 -3.75 180)
		(size 3 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Schrack-RT2-FormC-Dual-Coil_RM5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
