(footprint "Relay_NCR_HHG1D-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "NCR solid state relay 1A, 2A, 3A, 4A, https://ncr.hk/uploads/Relays/Solid_State_Relays/HHG1D-1.pdf")
	(tags "ssr")
	(property "Reference" "REF**"
		(at 14 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_NCR_HHG1D-1"
		(at 13.5 7.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 13.5 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 22 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 27 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_NCR_HHG1D.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
