(footprint "Relay_SPDT_Finder_40.11"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay SPDT Finder 40.11, 10/16A, 250V, body size 28.5x26.3mm, height 12.7mm, https://web.archive.org/web/20170816081018if_/https://www.finder-relais.net/de/finder-relais-serie-40.pdf")
	(tags "1-Form-C")
	(property "Reference" "REF**"
		(at 11.35 -4.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPDT_Finder_40.11"
		(at 11.35 24.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.35 10.6 0)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 20 7.5)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 16.5 0)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 23.5 0)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.08928571429)
	)
	(pad "A2" thru_hole circle
		(at 0 18)
		(size 2.8 2.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Finder_40.11.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
