(footprint "Relay_SPDT_Hongfa_HF3F-L-xx-1ZL1T"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hongfa subminature high power latching relay 5, 6, 9, 12, 24, 48VDC. 10A switching current, Form-C https://source.hongfa.com//Api/DownloadPdf/362")
	(tags "relays Hongfa form-c 1-coil ")
	(property "Reference" "REF**"
		(at -1.95 -2.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPDT_Hongfa_HF3F-L-xx-1ZL1T"
		(at 7.6 -5.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" "https://source.hongfa.com//Api/DownloadPdf/362"
		(at 5.2 15.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 12 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 6.2 6 0)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at -2 6)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 12.2 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 12.2 12)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1)
	)
	(pad "A2" thru_hole circle
		(at 0 12)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Hongfa_HF3F-L-xx-1ZL1T.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
