(footprint "Relay_SPDT_Panasonic_DR"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1 side stable, https://mediap.industry.panasonic.eu/assets/download-files/import/ds_dr_en_discon.pdf")
	(tags "nais single side")
	(property "Reference" "REF**"
		(at -2.667 -0.254 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPDT_Panasonic_DR"
		(at 8.89 2.54 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-"
		(at 5.588 -5.588 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "S+"
		(at 5.588 -1.016 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 9.525 -3.4925 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 17.78 0 180)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole rect
		(at 0 0 180)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 0 -7.62 180)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole circle
		(at 5.08 0 180)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A2" thru_hole circle
		(at 5.08 -7.62 180)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "PE" thru_hole circle
		(at 17.78 -7.62 180)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Panasonic_DR.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
