(footprint "Relay_SPDT_Panasonic_JW1_FormC"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Panasonic Relay SPDT, http://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_jw.pdf?via=ok")
	(tags "Panasonic Relay SPDT")
	(property "Reference" "REF**"
		(at 11.7 -11.55 180)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPDT_Panasonic_JW1_FormC"
		(at 12 3.9 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.6 -3.8 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 16.5 0 90)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 23.5 0 90)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 20 -7.6 90)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 0 -7.6 90)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Panasonic_JW1_FormC.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
