(footprint "Relay_SPDT_PotterBrumfield_T9AP5D52_12V30A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay SPDT Potter&Brumfield T9AP5D52 12V 30A 1xUn Connector Fast ON Only Dummy for Space NO Pads")
	(tags "Relay SPDT Potter&Brumfield T9AP5D52 12V 30A 1xUm Connector Fast ON Flachsteckeranschluss Only Dummy for Space NO Pads")
	(property "Reference" "REF**"
		(at 0 -4.25106 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPDT_PotterBrumfield_T9AP5D52_12V30A"
		(at 0 48.24894 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "11/C"
		(at -10.2743 17.84858 0)
		(layer "F.SilkS")
	)
	(fp_text user "A1"
		(at -8.57504 32.74822 0)
		(layer "F.SilkS")
	)
	(fp_text user "A2"
		(at 3.2512 32.79902 0)
		(layer "F.SilkS")
	)
	(fp_text user "12/NC"
		(at 6.85038 13.27404 0)
		(layer "F.SilkS")
	)
	(fp_text user "14/NO"
		(at 6.59892 21.79828 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 21.99894 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 3.50012 3.50012)
		(drill 3.50012)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 43.99788)
		(size 3.50012 3.50012)
		(drill 3.50012)
		(layers "*.Cu" "*.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_PotterBrumfield_T9AP5D52_12V30A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
