(footprint "Relay_SPDT_SANYOU_SRD_Series_Form_C"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
	(tags "relay Sanyu SRD form C")
	(property "Reference" "REF**"
		(at 8.1 9.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPDT_SANYOU_SRD_Series_Form_C"
		(at 8 -9.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.1 0.025 0)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at 0 -2.3 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0 90)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.95 6.05 90)
		(size 2.5 2.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 14.15 6.05 90)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 14.2 -6 90)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 1.95 -5.95 90)
		(size 2.5 2.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
