(footprint "Relay_SPST_Omron-G5Q-1A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay SPST-NO Omron Serie G5Q, http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5q.pdf")
	(tags "Relay SPST-NO Omron Serie G5Q")
	(property "Reference" "REF**"
		(at 9.5 -10.5 180)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPST_Omron-G5Q-1A"
		(at 8.8 3 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 9.6 -4.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10.16 0 180)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 17.78 0 180)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 -7.62 180)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_Omron-G5Q-1A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
